{
  "schema_version": "1.4.0",
  "id": "GHSA-q7v4-745g-qc2f",
  "modified": "2022-05-24T17:00:31Z",
  "published": "2022-05-24T17:00:31Z",
  "aliases": [
    "CVE-2019-10524"
  ],
  "details": "Lack of check for a negative value returned for get_clk is wrongly interpreted as valid pointer and lead to use after free in clk driver in Snapdragon Auto, Snapdragon Consumer IOT, Snapdragon Industrial IOT, Snapdragon Mobile, Snapdragon Voice & Music, Snapdragon Wearables in MDM9150, MDM9206, MDM9607, MDM9640, MDM9650, MSM8909W, MSM8996AU, QCS405, QCS605, Qualcomm 215, SD 210/SD 212/SD 205, SD 425, SD 427, SD 430, SD 435, SD 439 / SD 429, SD 450, SD 625, SD 632, SD 636, SD 665, SD 675, SD 712 / SD 710 / SD 670, SD 730, SD 820, SD 820A, SD 835, SD 845 / SD 850, SD 855, SDA660, SDM439, SDM630, SDM660, SDX20, SDX24",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2019-10524"
    },
    {
      "type": "WEB",
      "url": "https://source.android.com/security/bulletin"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-11-06T17:15:00Z"
  }
}