{
  "schema_version": "1.4.0",
  "id": "GHSA-qcj5-h89x-f3cj",
  "modified": "2022-05-24T16:52:42Z",
  "published": "2022-05-24T16:52:42Z",
  "aliases": [
    "CVE-2019-5999"
  ],
  "details": "Buffer overflow in PTP (Picture Transfer Protocol) of EOS series digital cameras (EOS-1D X firmware version 2.1.0 and earlier, EOS-1D X MKII firmware version 1.1.6 and earlier, EOS-1D C firmware version 1.4.1 and earlier, EOS 5D MARK III firmware version 1.3.5 and earlier, EOS 5D MARK IV firmware version 1.2.0 and earlier, EOS 5DS firmware version 1.1.2 and earlier, EOS 5DS R firmware version 1.1.2 and earlier, EOS 6D firmware version 1.1.8 and earlier, EOS 6D MARK II firmware version 1.0.4 and earlier, EOS 7D MARK II firmware version 1.1.2 and earlier, EOS 70 D firmware version 1.1.2 and earlier, EOS 80 D firmware version 1.0.2 and earlier, EOS KISS X7I / EOS D REBEL T5I / EOS 700D firmware version 1.1.5 and earlier, EOS KISS X8I / EOS D REBEL T6I / EOS 750D firmware version 1.0.0 and earlier, EOS KISS X9I / EOS D REBEL T7I / EOS 800D firmware version 1.0.1 and earlier, EOS KISS X7 / EOS D REBEL SL1 / EOS 100D firmware version 1.0.1 and earlier, EOS KISS X9 / EOS D REBEL SL2 / EOS 200D firmware version 1.0.1 and earlier, EOS KISS X10 / EOS D REBEL SL3 / EOS 200D / EOS 250D firmware version 1.0.1 and earlier, EOS 8000D / EOS D REBEL T6S / EOS 760D firmware version 1.0.0 and earlier, EOS 9000D / EOS 77D firmware version 1.0.2 and earlier, EOS KISS X70 / EOS D REBEL T5 / EOS 1200D firmware version 1.0.2 and earlier, EOS D REBEL T5 RE / EOS 1200D MG / EOS HI firmware version 1.0.2 and earlier, EOS KISS X80 / EOS D REBEL T6 / EOS 1300D firmware version 1.1.0 and earlier, EOS KISS X90 / EOS D REBEL T7 / EOS 1500D / EOS 2000D firmware version 1.0.0 and earlier, EOS D REBEL T100 / EOS 3000D / EOS 4000D firmware version 1.0.0 and earlier, EOS R firmware version 1.3.0 and earlier, EOS RP firmware version 1.2.0 and earlier, EOS RP GOLD firmware version 1.2.0 and earlier, EOS M2 firmware version 1.0.3 and earlier, EOS M3 firmware version 1.2.0 and earlier, EOS M5 firmware version 1.0.1 and earlier, EOS M6 firmware version 1.0.1 and earlier, EOS M6(China) firmware version 5.0.0 and earlier, EOS M10 firmware version 1.1.0 and earlier, EOS M100 firmware version 1.0.0 and earlier, EOS KISS M / EOS M50 firmware version 1.0.2 and earlier) and PowerShot SX740 HS firmware version 1.0.1 and earlier, PowerShot SX70 HS firmware version 1.1.0 and earlier, and PowerShot G5Xmark? firmware version 1.0.1 and earlier allows an attacker on the same network segment to trigger the affected product being unresponsive or to execute arbitrary code on the affected product via blerequest command.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2019-5999"
    },
    {
      "type": "WEB",
      "url": "https://cweb.canon.jp/e-support/products/eos-d/190806dilc-firm.html"
    },
    {
      "type": "WEB",
      "url": "https://research.checkpoint.com/say-cheese-ransomware-ing-a-dslr-camera"
    },
    {
      "type": "WEB",
      "url": "https://www.canon-europe.com/support/product-security"
    },
    {
      "type": "WEB",
      "url": "https://www.usa.canon.com/internet/portal/us/home/support/product-advisories/detail/the-vulnerability-in-canon-digital-cameras"
    },
    {
      "type": "WEB",
      "url": "http://jvn.jp/en/vu/JVNVU97511331/index.html"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-08-06T19:15:00Z"
  }
}