# SPDX-License-Identifier: GPL-2.0-only
config DRM_I2C_ADV7511
	tristate "ADV7511 encoder"
	depends on OF
	select DRM_KMS_HELPER
	select REGMAP_I2C
	select DRM_MIPI_DSI
	select DRM_DISPLAY_HELPER
	select DRM_BRIDGE_CONNECTOR
	select DRM_DISPLAY_HDMI_STATE_HELPER
	help
	  Support for the Analog Devices ADV7511(W)/13/33/35 HDMI encoders.

config DRM_I2C_ADV7511_AUDIO
	bool "ADV7511 HDMI Audio driver"
	depends on DRM_I2C_ADV7511 && SND_SOC
	select SND_SOC_HDMI_CODEC
	help
	  Support the ADV7511 HDMI Audio interface. This is used in
	  conjunction with the AV7511  HDMI driver.

config DRM_I2C_ADV7511_CEC
	bool "ADV7511/33/35 HDMI CEC driver"
	depends on DRM_I2C_ADV7511
	select DRM_DISPLAY_HDMI_CEC_HELPER
	default y
	help
	  When selected the HDMI transmitter will support the CEC feature.
