# SPDX-License-Identifier: GPL-2.0-only
config DRM_ASPEED_GFX
	tristate "ASPEED BMC Display Controller"
	depends on DRM && OF
	depends on (COMPILE_TEST || ARCH_ASPEED)
	depends on MMU
	select DRM_CLIENT_SELECTION
	select DRM_KMS_HELPER
	select DRM_GEM_DMA_HELPER
	select DMA_CMA if HAVE_DMA_CONTIGUOUS
	select CMA if HAVE_DMA_CONTIGUOUS
	select MFD_SYSCON
	help
	  Chose this option if you have an ASPEED AST2500 SOC Display
	  Controller (aka GFX).

	  If M is selected this module will be called aspeed_gfx.
