# SPDX-License-Identifier: GPL-2.0-only
config DRM_AST
	tristate "AST server chips"
	depends on DRM && PCI
	select DRM_CLIENT_SELECTION
	select DRM_GEM_SHMEM_HELPER
	select DRM_KMS_HELPER
	select I2C
	select I2C_ALGOBIT
	help
	 Say yes for experimental AST GPU driver. Do not enable
	 this driver without having a working -modesetting,
	 and a version of AST that knows to fail if KMS
	 is bound to the driver. These GPUs are commonly found
	 in server chipsets.

