# SPDX-License-Identifier: GPL-2.0-only
config DRM_MXS
	bool
	help
	  Choose this option to select drivers for MXS FB devices

config DRM_MXSFB
	tristate "i.MX (e)LCDIF LCD controller"
	depends on DRM && OF
	depends on COMMON_CLK
	depends on ARCH_MXS || ARCH_MXC || COMPILE_TEST
	select DRM_CLIENT_SELECTION
	select DRM_MXS
	select DRM_KMS_HELPER
	select DRM_GEM_DMA_HELPER
	select DRM_PANEL
	select DRM_PANEL_BRIDGE
	help
	  Choose this option if you have an LCDIF or eLCDIF LCD controller.
	  Those devices are found in various i.MX SoC (including i.MX23,
	  i.MX28, i.MX6SX, i.MX7 and i.MX8M).

	  If M is selected the module will be called mxsfb.

config DRM_IMX_LCDIF
	tristate "i.MX LCDIFv3 LCD controller"
	depends on DRM && OF
	depends on COMMON_CLK
	depends on ARCH_MXC || COMPILE_TEST
	select DRM_CLIENT_SELECTION
	select DRM_MXS
	select DRM_KMS_HELPER
	select DRM_GEM_DMA_HELPER
	select DRM_PANEL
	select DRM_PANEL_BRIDGE
	help
	  Choose this option if you have an LCDIFv3 LCD controller.
	  Those devices are found in various i.MX SoC (i.MX8MP,
	  i.MXRT).

	  If M is selected the module will be called imx-lcdif.
