# Function _mm512_shldi_epi32

1.89.0 · Source

    pub fn _mm512_shldi_epi32(a: __m512i, b: __m512i, const IMM8: i32) -> __m512i

Available on (x86 or x86-64) and target feature `avx512vbmi2` and x86-64 only.
Expand description

Concatenate packed 32-bit integers in a and b producing an intermediate 64-bit result. Shift the result left by imm8 bits, and store the upper 32-bits in dst.

Intel’s documentation