# Function _mm512_mask_srl_epi32

1.89.0 · Source

    pub fn _mm512_mask_srl_epi32(
        src: __m512i,
        k: __mmask16,
        a: __m512i,
        count: __m128i,
    ) -> __m512i

Available on (x86 or x86-64) and target feature `avx512f` and x86-64 only.
Expand description

Shift packed 32-bit integers in a right by count while shifting in zeros, and store the results in dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation