# Function _mm512_permutevar_epi32

1.89.0 · Source

    pub fn _mm512_permutevar_epi32(idx: __m512i, a: __m512i) -> __m512i

Available on (x86 or x86-64) and target feature `avx512f` and x86-64 only.
Expand description

Shuffle 32-bit integers in a across lanes using the corresponding index in idx, and store the results in dst. Note that this intrinsic shuffles across 128-bit lanes, unlike past intrinsics that use the permutevar name. This intrinsic is identical to _mm512_permutexvar_epi32, and it is recommended that you use that intrinsic name.

Intel’s documentation