# Function _mm512_maskz_mulhi_epu16

1.89.0 · Source

    pub fn _mm512_maskz_mulhi_epu16(k: __mmask32, a: __m512i, b: __m512i) -> __m512i

Available on (x86 or x86-64) and target feature `avx512bw` and x86-64 only.
Expand description

Multiply the packed unsigned 16-bit integers in a and b, producing intermediate 32-bit integers, and store the high 16 bits of the intermediate integers in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation