# Function _mm_maskz_broadcastw_epi16

1.89.0 · Source

    pub fn _mm_maskz_broadcastw_epi16(k: __mmask8, a: __m128i) -> __m128i

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86 only.
Expand description

Broadcast the low packed 16-bit integer from a to all elements of dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation