# Function _mm_maskz_max_epi16

1.89.0 · Source

    pub fn _mm_maskz_max_epi16(k: __mmask8, a: __m128i, b: __m128i) -> __m128i

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86 only.
Expand description

Compare packed signed 16-bit integers in a and b, and store packed maximum values in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation