# Function _mm512_maskz_shrdv_epi16

1.89.0 · Source

    pub fn _mm512_maskz_shrdv_epi16(
        k: __mmask32,
        a: __m512i,
        b: __m512i,
        c: __m512i,
    ) -> __m512i

Available on (x86 or x86-64) and target feature `avx512vbmi2` and x86-64 only.
Expand description

Concatenate packed 16-bit integers in b and a producing an intermediate 32-bit result. Shift the result right by the amount specified in the corresponding element of c, and store the lower 16-bits in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation