# Function _mm256_mask_broadcastw_epi16

1.89.0 · Source

    pub fn _mm256_mask_broadcastw_epi16(
        src: __m256i,
        k: __mmask16,
        a: __m128i,
    ) -> __m256i

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86-64 only.
Expand description

Broadcast the low packed 16-bit integer from a to all elements of dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation