# Function _mm256_mask_srlv_epi16

1.89.0 · Source

    pub fn _mm256_mask_srlv_epi16(
        src: __m256i,
        k: __mmask16,
        a: __m256i,
        count: __m256i,
    ) -> __m256i

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86 only.
Expand description

Shift packed 16-bit integers in a right by the amount specified by the corresponding element in count while shifting in zeros, and store the results in dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation