# Function _mm256_maskz_shldv_epi16

1.89.0 · Source

    pub fn _mm256_maskz_shldv_epi16(
        k: __mmask16,
        a: __m256i,
        b: __m256i,
        c: __m256i,
    ) -> __m256i

Available on (x86 or x86-64) and target feature `avx512vbmi2` and target feature `avx512vl` and x86 only.
Expand description

Concatenate packed 16-bit integers in a and b producing an intermediate 32-bit result. Shift the result left by the amount specified in the corresponding element of c, and store the upper 16-bits in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation