# Function _mm512_maskz_cvtepu8_epi16

1.89.0 · Source

    pub fn _mm512_maskz_cvtepu8_epi16(k: __mmask32, a: __m256i) -> __m512i

Available on (x86 or x86-64) and target feature `avx512bw` and x86 only.
Expand description

Zero extend packed unsigned 8-bit integers in a to packed 16-bit integers, and store the results in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation