# Function _mm512_mask_madd_epi16

1.89.0 · Source

    pub fn _mm512_mask_madd_epi16(
        src: __m512i,
        k: __mmask16,
        a: __m512i,
        b: __m512i,
    ) -> __m512i

Available on (x86 or x86-64) and target feature `avx512bw` and x86-64 only.
Expand description

Multiply packed signed 16-bit integers in a and b, producing intermediate signed 32-bit integers. Horizontally add adjacent pairs of intermediate 32-bit integers, and pack the results in dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation