# Function _mm256_shufflehi_epi16

1.27.0 · Source

    pub fn _mm256_shufflehi_epi16(a: __m256i, const IMM8: i32) -> __m256i

Available on (x86 or x86-64) and target feature `avx2` and x86-64 only.
Expand description

Shuffles 16-bit integers in the high 64 bits of 128-bit lanes of `a` using the control in `imm8`. The low 64 bits of 128-bit lanes of `a` are copied to the output.

Intel’s documentation