# Function _mm256_shrdi_epi16

1.89.0 · Source

    pub fn _mm256_shrdi_epi16(a: __m256i, b: __m256i, const IMM8: i32) -> __m256i

Available on (x86 or x86-64) and target feature `avx512vbmi2` and target feature `avx512vl` and x86-64 only.
Expand description

Concatenate packed 16-bit integers in b and a producing an intermediate 32-bit result. Shift the result right by imm8 bits, and store the lower 16-bits in dst.

Intel’s documentation