# Function _mm512_shufflehi_epi16

1.89.0 · Source

    pub fn _mm512_shufflehi_epi16(a: __m512i, const IMM8: i32) -> __m512i

Available on (x86 or x86-64) and target feature `avx512bw` and x86 only.
Expand description

Shuffle 16-bit integers in the high 64 bits of 128-bit lanes of a using the control in imm8. Store the results in the high 64 bits of 128-bit lanes of dst, with the low 64 bits of 128-bit lanes being copied from a to dst.

Intel’s documentation