# Function _mm256_mask_shufflehi_epi16

1.89.0 · Source

    pub fn _mm256_mask_shufflehi_epi16(
        src: __m256i,
        k: __mmask16,
        a: __m256i,
        const IMM8: i32,
    ) -> __m256i

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86-64 only.
Expand description

Shuffle 16-bit integers in the high 64 bits of 128-bit lanes of a using the control in imm8. Store the results in the high 64 bits of 128-bit lanes of dst, with the low 64 bits of 128-bit lanes being copied from a to dst, using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation