# Function _mm512_maskz_expand_epi16

1.89.0 · Source

    pub fn _mm512_maskz_expand_epi16(k: __mmask32, a: __m512i) -> __m512i

Available on (x86 or x86-64) and target feature `avx512vbmi2` and x86-64 only.
Expand description

Load contiguous active 16-bit integers from a (those with their respective bit set in mask k), and store the results in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation