# Function _mm512_maskz_unpacklo_epi16

1.89.0 · Source

    pub fn _mm512_maskz_unpacklo_epi16(
        k: __mmask32,
        a: __m512i,
        b: __m512i,
    ) -> __m512i

Available on (x86 or x86-64) and target feature `avx512bw` and x86 only.
Expand description

Unpack and interleave 16-bit integers from the low half of each 128-bit lane in a and b, and store the results in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation