# Function _mm512_maskz_min_epi16

1.89.0 · Source

    pub fn _mm512_maskz_min_epi16(k: __mmask32, a: __m512i, b: __m512i) -> __m512i

Available on (x86 or x86-64) and target feature `avx512bw` and x86-64 only.
Expand description

Compare packed signed 16-bit integers in a and b, and store packed minimum values in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation