# Function _mm256_maskz_permutexvar_epi16

1.89.0 · Source

    pub fn _mm256_maskz_permutexvar_epi16(
        k: __mmask16,
        idx: __m256i,
        a: __m256i,
    ) -> __m256i

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86 only.
Expand description

Shuffle 16-bit integers in a across lanes using the corresponding index in idx, and store the results in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation