# Function _mm_mask_sll_epi16

1.89.0 · Source

    pub fn _mm_mask_sll_epi16(
        src: __m128i,
        k: __mmask8,
        a: __m128i,
        count: __m128i,
    ) -> __m128i

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86-64 only.
Expand description

Shift packed 16-bit integers in a left by count while shifting in zeros, and store the results in dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation