ndrej Jirman <megi@xff.cz>
Signed-off-by: Rudraksha Gupta <guptarud@gmail.com>
Reviewed-by: Pavel Machek <pavel@ucw.cz>
Link: https://patch.msgid.link/20251124-ppp_light_accel_mag_vol-down-v5-4-f9a10a0a50eb@gmail.com
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts |    4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts
@@ -40,13 +40,13 @@
 		button-up {
 			label = "Volume Up";
 			linux,code = <KEY_VOLUMEUP>;
-			press-threshold-microvolt = <100000>;
+			press-threshold-microvolt = <2000>;
 		};
 
 		button-down {
 			label = "Volume Down";
 			linux,code = <KEY_VOLUMEDOWN>;
-			press-threshold-microvolt = <600000>;
+			press-threshold-microvolt = <300000>;
 		};
 	};
 [PATCH 6.12 053/169] arm64: dts: rockchip: Fix voltage threshold for volume keys for Pinephone ProGreg Kroah-Hartman <gregkh@linuxfoundation.org> undefinedstable@vger.kernel.org undefined undefined undefined undefined undefined undefined“…Í6
