# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
%YAML 1.2
---
$id: http://devicetree.org/schemas/timer/csky,mptimer.yaml#
$schema: http://devicetree.org/meta-schemas/core.yaml#

title: C-SKY Multi-processors Timer

maintainers:
  - Flavio Suligoi <f.suligoi@asem.it>
  - Guo Ren <guoren@kernel.org>

description: |
  C-SKY multi-processors timer is designed for C-SKY SMP system and the regs are
  accessed by cpu co-processor 4 registers with mtcr/mfcr.

   - PTIM_CTLR "cr<0, 14>" Control reg to start reset timer.
   - PTIM_TSR  "cr<1, 14>" Interrupt cleanup status reg.
   - PTIM_CCVR "cr<3, 14>" Current counter value reg.
   - PTIM_LVR  "cr<6, 14>" Window value reg to trigger next event.

properties:
  compatible:
    items:
      - const: csky,mptimer

  clocks:
    maxItems: 1

  interrupts:
    maxItems: 1

required:
  - compatible
  - clocks
  - interrupts

additionalProperties: false

examples:
  - |
    timer {
        compatible = "csky,mptimer";
        clocks = <&dummy_apb_clk>;
        interrupts = <16>;
    };
