# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
%YAML 1.2
---
$id: http://devicetree.org/schemas/usb/brcm,bdc.yaml#
$schema: http://devicetree.org/meta-schemas/core.yaml#

title: Broadcom USB Device Controller (BDC)

maintainers:
  - Al Cooper <alcooperx@gmail.com>
  - Florian Fainelli <f.fainelli@gmail.com>

properties:
  compatible:
    items:
      - enum:
          - brcm,bdc-udc-v2
          - brcm,bdc

  reg:
    maxItems: 1

  interrupts:
    maxItems: 1

  phys:
    minItems: 1
    items:
      - description: USB 2.0 or 3.0 PHY
      - description: USB 3.0 PHY if there is a dedicated 2.0 PHY

  clocks:
    maxItems: 1

required:
  - compatible
  - reg
  - interrupts

additionalProperties: false

examples:
  - |
    usb@f0b02000 {
        compatible = "brcm,bdc-udc-v2";
        reg = <0xf0b02000 0xfc4>;
        interrupts = <0x0 0x60 0x0>;
        phys = <&usbphy_0 0x0>;
        clocks = <&sw_usbd>;
    };
