# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
%YAML 1.2
---
$id: http://devicetree.org/schemas/timestamp/hte-consumer.yaml#
$schema: http://devicetree.org/meta-schemas/core.yaml#

title: HTE Consumer

maintainers:
  - Dipen Patel <dipenp@nvidia.com>

select: true

properties:
  timestamps:
    $ref: /schemas/types.yaml#/definitions/phandle-array
    description:
      The list of HTE provider phandle. The first cell must represent the
      provider phandle followed by the line identifiers. The meaning of the
      line identifier and exact number of arguments must be specified in the
      HTE provider device tree binding document.

  timestamp-names:
    $ref: /schemas/types.yaml#/definitions/string-array
    description:
      An optional string property to label each line specifier present in the
      timestamp property.

dependencies:
  timestamp-names: [ timestamps ]

additionalProperties: true

examples:
  - |
    hte_tegra_consumer {
              timestamps = <&tegra_hte_aon 0x9>, <&tegra_hte_lic 0x19>;
              timestamp-names = "hte-gpio", "hte-i2c";
    };
