# SPDX-License-Identifier: (GPL-2.0 OR BSD-2-Clause)
%YAML 1.2
---
$id: http://devicetree.org/schemas/usb/qcom,dwc3.yaml#
$schema: http://devicetree.org/meta-schemas/core.yaml#

title: Legacy Qualcomm SuperSpeed DWC3 USB SoC controller

maintainers:
  - Wesley Cheng <quic_wcheng@quicinc.com>

# Use the combined qcom,snps-dwc3 instead
deprecated: true

select:
  properties:
    compatible:
      contains:
        const: qcom,dwc3
  required:
    - compatible

properties:
  compatible:
    items:
      - enum:
          - qcom,ipq4019-dwc3
          - qcom,ipq5018-dwc3
          - qcom,ipq5332-dwc3
          - qcom,ipq5424-dwc3
          - qcom,ipq6018-dwc3
          - qcom,ipq8064-dwc3
          - qcom,ipq8074-dwc3
          - qcom,ipq9574-dwc3
          - qcom,msm8953-dwc3
          - qcom,msm8994-dwc3
          - qcom,msm8996-dwc3
          - qcom,msm8998-dwc3
          - qcom,qcm2290-dwc3
          - qcom,qcs404-dwc3
          - qcom,qcs615-dwc3
          - qcom,qcs8300-dwc3
          - qcom,qdu1000-dwc3
          - qcom,sa8775p-dwc3
          - qcom,sar2130p-dwc3
          - qcom,sc7180-dwc3
          - qcom,sc7280-dwc3
          - qcom,sc8180x-dwc3
          - qcom,sc8180x-dwc3-mp
          - qcom,sc8280xp-dwc3
          - qcom,sc8280xp-dwc3-mp
          - qcom,sdm660-dwc3
          - qcom,sdm670-dwc3
          - qcom,sdm845-dwc3
          - qcom,sdx55-dwc3
          - qcom,sdx65-dwc3
          - qcom,sdx75-dwc3
          - qcom,sm4250-dwc3
          - qcom,sm6115-dwc3
          - qcom,sm6125-dwc3
          - qcom,sm6350-dwc3
          - qcom,sm6375-dwc3
          - qcom,sm8150-dwc3
          - qcom,sm8250-dwc3
          - qcom,sm8350-dwc3
          - qcom,sm8450-dwc3
          - qcom,sm8550-dwc3
          - qcom,sm8650-dwc3
          - qcom,sm8750-dwc3
          - qcom,x1e80100-dwc3
          - qcom,x1e80100-dwc3-mp
      - const: qcom,dwc3

  reg:
    description: Offset and length of register set for QSCRATCH wrapper
    maxItems: 1

  "#address-cells":
    enum: [ 1, 2 ]

  "#size-cells":
    enum: [ 1, 2 ]

  ranges: true

  power-domains:
    description: specifies a phandle to PM domain provider node
    maxItems: 1

  required-opps:
    maxItems: 1

  clocks:
    description: |
      Several clocks are used, depending on the variant. Typical ones are::
       - cfg_noc:: System Config NOC clock.
       - core:: Master/Core clock, has to be >= 125 MHz for SS operation and >=
                60MHz for HS operation.
       - iface:: System bus AXI clock.
       - sleep:: Sleep clock, used for wakeup when USB3 core goes into low
                 power mode (U3).
       - mock_utmi:: Mock utmi clock needed for ITP/SOF generation in host
                     mode. Its frequency should be 19.2MHz.
    minItems: 1
    maxItems: 9

  clock-names:
    minItems: 1
    maxItems: 9

  resets:
    maxItems: 1

  interconnects:
    maxItems: 2

  interconnect-names:
    items:
      - const: usb-ddr
      - const: apps-usb

  interrupts:
    description: |
      Different types of interrupts are used based on HS PHY used on target:
        - pwr_event: Used for wakeup based on other power events.
        - hs_phy_irq: Apart from DP/DM/QUSB2 PHY interrupts, there is
                       hs_phy_irq which is not triggered by default and its
                       functionality is mutually exclusive to that of
                       {dp/dm}_hs_phy_irq and qusb2_phy_irq.
        - qusb2_phy: SoCs with QUSB2 PHY do not have separate DP/DM IRQs and
                      expose only a single IRQ whose behavior can be modified
                      by the QUSB2PHY_INTR_CTRL register. The required DPSE/
                      DMSE configuration is done in QUSB2PHY_INTR_CTRL register
                      of PHY address space.
        - {dp/dm}_hs_phy_irq: These IRQ's directly reflect changes on the DP/
                               DM pads of the SoC. These are used for wakeup
                               only on SoCs with non-QUSB2 targets with
                               exception of SDM670/SDM845/SM6350.
        - ss_phy_irq: Used for remote wakeup in Super Speed mode of operation.
    minItems: 2
    maxItems: 18

  interrupt-names:
    minItems: 2
    maxItems: 18

  qcom,select-utmi-as-pipe-clk:
    description:
      If present, disable USB3 pipe_clk requirement.
      Used when dwc3 operates without SSPHY and only
      HS/FS/LS modes are supported.
    type: boolean

  wakeup-source: true

# Required child node:

patternProperties:
  "^usb@[0-9a-f]+$":
    $ref: snps,dwc3.yaml#
    unevaluatedProperties: false

    properties:
      wakeup-source: false

required:
  - compatible
  - reg
  - "#address-cells"
  - "#size-cells"
  - ranges
  - clocks
  - clock-names
  - interrupts
  - interrupt-names

allOf:
  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,ipq4019-dwc3
              - qcom,ipq5332-dwc3
    then:
      properties:
        clocks:
          maxItems: 3
        clock-names:
          items:
            - const: core
            - const: sleep
            - const: mock_utmi

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,ipq8064-dwc3
    then:
      properties:
        clocks:
          items:
            - description: Master/Core clock, has to be >= 125 MHz
                for SS operation and >= 60MHz for HS operation.
        clock-names:
          items:
            - const: core

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,ipq9574-dwc3
              - qcom,msm8953-dwc3
              - qcom,msm8996-dwc3
              - qcom,msm8998-dwc3
              - qcom,qcs8300-dwc3
              - qcom,sa8775p-dwc3
              - qcom,sc7180-dwc3
              - qcom,sc7280-dwc3
              - qcom,sdm670-dwc3
              - qcom,sdm845-dwc3
              - qcom,sdx55-dwc3
              - qcom,sdx65-dwc3
              - qcom,sdx75-dwc3
              - qcom,sm6350-dwc3
    then:
      properties:
        clocks:
          maxItems: 5
        clock-names:
          items:
            - const: cfg_noc
            - const: core
            - const: iface
            - const: sleep
            - const: mock_utmi

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,ipq6018-dwc3
    then:
      properties:
        clocks:
          minItems: 3
          maxItems: 4
        clock-names:
          oneOf:
            - items:
                - const: core
                - const: sleep
                - const: mock_utmi
            - items:
                - const: cfg_noc
                - const: core
                - const: sleep
                - const: mock_utmi

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,ipq8074-dwc3
              - qcom,qdu1000-dwc3
    then:
      properties:
        clocks:
          maxItems: 4
        clock-names:
          items:
            - const: cfg_noc
            - const: core
            - const: sleep
            - const: mock_utmi

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,ipq5018-dwc3
              - qcom,msm8994-dwc3
              - qcom,qcs404-dwc3
    then:
      properties:
        clocks:
          maxItems: 4
        clock-names:
          items:
            - const: core
            - const: iface
            - const: sleep
            - const: mock_utmi

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,sc8280xp-dwc3
              - qcom,sc8280xp-dwc3-mp
              - qcom,x1e80100-dwc3
              - qcom,x1e80100-dwc3-mp
    then:
      properties:
        clocks:
          maxItems: 9
        clock-names:
          items:
            - const: cfg_noc
            - const: core
            - const: iface
            - const: sleep
            - const: mock_utmi
            - const: noc_aggr
            - const: noc_aggr_north
            - const: noc_aggr_south
            - const: noc_sys

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,sdm660-dwc3
    then:
      properties:
        clocks:
          minItems: 4
          maxItems: 5
        clock-names:
          oneOf:
            - items:
                - const: cfg_noc
                - const: core
                - const: iface
                - const: sleep
                - const: mock_utmi
            - items:
                - const: cfg_noc
                - const: core
                - const: sleep
                - const: mock_utmi

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,qcm2290-dwc3
              - qcom,qcs615-dwc3
              - qcom,sar2130p-dwc3
              - qcom,sc8180x-dwc3
              - qcom,sc8180x-dwc3-mp
              - qcom,sm6115-dwc3
              - qcom,sm6125-dwc3
              - qcom,sm8150-dwc3
              - qcom,sm8250-dwc3
              - qcom,sm8450-dwc3
              - qcom,sm8550-dwc3
              - qcom,sm8650-dwc3
              - qcom,sm8750-dwc3
    then:
      properties:
        clocks:
          minItems: 6
        clock-names:
          items:
            - const: cfg_noc
            - const: core
            - const: iface
            - const: sleep
            - const: mock_utmi
            - const: xo

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,sm8350-dwc3
    then:
      properties:
        clocks:
          minItems: 5
          maxItems: 6
        clock-names:
          minItems: 5
          items:
            - const: cfg_noc
            - const: core
            - const: iface
            - const: sleep
            - const: mock_utmi
            - const: xo

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,ipq5018-dwc3
              - qcom,ipq6018-dwc3
              - qcom,ipq8074-dwc3
              - qcom,msm8953-dwc3
              - qcom,msm8998-dwc3
    then:
      properties:
        interrupts:
          minItems: 2
          maxItems: 3
        interrupt-names:
          minItems: 2
          items:
            - const: pwr_event
            - const: qusb2_phy
            - const: ss_phy_irq

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,msm8996-dwc3
              - qcom,qcs404-dwc3
              - qcom,sdm660-dwc3
              - qcom,sm6115-dwc3
              - qcom,sm6125-dwc3
    then:
      properties:
        interrupts:
          minItems: 3
          maxItems: 4
        interrupt-names:
          minItems: 3
          items:
            - const: pwr_event
            - const: qusb2_phy
            - const: hs_phy_irq
            - const: ss_phy_irq

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,ipq5332-dwc3
    then:
      properties:
        interrupts:
          maxItems: 3
        interrupt-names:
          items:
            - const: pwr_event
            - const: dp_hs_phy_irq
            - const: dm_hs_phy_irq

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,x1e80100-dwc3
    then:
      properties:
        interrupts:
          minItems: 3
          maxItems: 4
        interrupt-names:
          minItems: 3
          items:
            - const: pwr_event
            - const: dp_hs_phy_irq
            - const: dm_hs_phy_irq
            - const: ss_phy_irq

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,ipq4019-dwc3
              - qcom,ipq8064-dwc3
              - qcom,msm8994-dwc3
              - qcom,qcs615-dwc3
              - qcom,qcs8300-dwc3
              - qcom,qdu1000-dwc3
              - qcom,sa8775p-dwc3
              - qcom,sc7180-dwc3
              - qcom,sc7280-dwc3
              - qcom,sc8180x-dwc3
              - qcom,sc8280xp-dwc3
              - qcom,sdm670-dwc3
              - qcom,sdm845-dwc3
              - qcom,sdx55-dwc3
              - qcom,sdx65-dwc3
              - qcom,sdx75-dwc3
              - qcom,sm4250-dwc3
              - qcom,sm6350-dwc3
              - qcom,sm8150-dwc3
              - qcom,sm8250-dwc3
              - qcom,sm8350-dwc3
              - qcom,sm8450-dwc3
              - qcom,sm8550-dwc3
              - qcom,sm8650-dwc3
              - qcom,sm8750-dwc3
    then:
      properties:
        interrupts:
          minItems: 4
          maxItems: 5
        interrupt-names:
          minItems: 4
          items:
            - const: pwr_event
            - const: hs_phy_irq
            - const: dp_hs_phy_irq
            - const: dm_hs_phy_irq
            - const: ss_phy_irq

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,sc8180x-dwc3-mp
              - qcom,x1e80100-dwc3-mp
    then:
      properties:
        interrupts:
          minItems: 10
          maxItems: 10
        interrupt-names:
          items:
            - const: pwr_event_1
            - const: pwr_event_2
            - const: hs_phy_1
            - const: hs_phy_2
            - const: dp_hs_phy_1
            - const: dm_hs_phy_1
            - const: dp_hs_phy_2
            - const: dm_hs_phy_2
            - const: ss_phy_1
            - const: ss_phy_2

  - if:
      properties:
        compatible:
          contains:
            enum:
              - qcom,sc8280xp-dwc3-mp
    then:
      properties:
        interrupts:
          minItems: 18
          maxItems: 18
        interrupt-names:
          items:
            - const: pwr_event_1
            - const: pwr_event_2
            - const: pwr_event_3
            - const: pwr_event_4
            - const: hs_phy_1
            - const: hs_phy_2
            - const: hs_phy_3
            - const: hs_phy_4
            - const: dp_hs_phy_1
            - const: dm_hs_phy_1
            - const: dp_hs_phy_2
            - const: dm_hs_phy_2
            - const: dp_hs_phy_3
            - const: dm_hs_phy_3
            - const: dp_hs_phy_4
            - const: dm_hs_phy_4
            - const: ss_phy_1
            - const: ss_phy_2

additionalProperties: false

examples:
  - |
    #include <dt-bindings/clock/qcom,gcc-sdm845.h>
    #include <dt-bindings/interrupt-controller/arm-gic.h>
    #include <dt-bindings/interrupt-controller/irq.h>
    soc {
        #address-cells = <2>;
        #size-cells = <2>;

        usb@a6f8800 {
            compatible = "qcom,sdm845-dwc3", "qcom,dwc3";
            reg = <0 0x0a6f8800 0 0x400>;

            #address-cells = <2>;
            #size-cells = <2>;
            ranges;
            clocks = <&gcc GCC_CFG_NOC_USB3_PRIM_AXI_CLK>,
                     <&gcc GCC_USB30_PRIM_MASTER_CLK>,
                     <&gcc GCC_AGGRE_USB3_PRIM_AXI_CLK>,
                     <&gcc GCC_USB30_PRIM_SLEEP_CLK>,
                     <&gcc GCC_USB30_PRIM_MOCK_UTMI_CLK>;
            clock-names = "cfg_noc",
                          "core",
                          "iface",
                          "sleep",
                          "mock_utmi";

            assigned-clocks = <&gcc GCC_USB30_PRIM_MOCK_UTMI_CLK>,
                          <&gcc GCC_USB30_PRIM_MASTER_CLK>;
            assigned-clock-rates = <19200000>, <150000000>;

            interrupts = <GIC_SPI 130 IRQ_TYPE_LEVEL_HIGH>,
                         <GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>,
                         <GIC_SPI 489 IRQ_TYPE_EDGE_BOTH>,
                         <GIC_SPI 488 IRQ_TYPE_EDGE_BOTH>,
                         <GIC_SPI 486 IRQ_TYPE_LEVEL_HIGH>;
            interrupt-names = "pwr_event", "hs_phy_irq",
                          "dp_hs_phy_irq", "dm_hs_phy_irq", "ss_phy_irq";

            power-domains = <&gcc USB30_PRIM_GDSC>;

            resets = <&gcc GCC_USB30_PRIM_BCR>;

            usb@a600000 {
                compatible = "snps,dwc3";
                reg = <0 0x0a600000 0 0xcd00>;
                interrupts = <GIC_SPI 133 IRQ_TYPE_LEVEL_HIGH>;
                iommus = <&apps_smmu 0x740 0>;
                snps,dis_u2_susphy_quirk;
                snps,dis_enblslpm_quirk;
                phys = <&usb_1_hsphy>, <&usb_1_ssphy>;
                phy-names = "usb2-phy", "usb3-phy";
            };
        };
    };
