# SPDX-License-Identifier: GPL-2.0
%YAML 1.2
---
$id: http://devicetree.org/schemas/usb/snps,dwc3-common.yaml#
$schema: http://devicetree.org/meta-schemas/core.yaml#

title: Synopsys DesignWare USB3 Controller common properties

maintainers:
  - Felipe Balbi <balbi@kernel.org>

description:
  Defines the properties of the DWC3 core as being embedded in either an
  vendor-specific implementation or as a standalone component.

allOf:
  - $ref: usb-drd.yaml#
  - if:
      properties:
        dr_mode:
          const: peripheral

      required:
        - dr_mode
    then:
      $ref: usb.yaml#
    else:
      $ref: usb-xhci.yaml#

properties:
  extcon:
    maxItems: 1
    deprecated: true

  usb-phy:
    minItems: 1
    items:
      - description: USB2/HS PHY
      - description: USB3/SS PHY

  phys:
    minItems: 1
    maxItems: 19

  phy-names:
    minItems: 1
    maxItems: 19
    oneOf:
      - items:
          enum: [ usb2-phy, usb3-phy ]
      - items:
          pattern: "^usb(2-([0-9]|1[0-4])|3-[0-3])$"

  snps,usb2-lpm-disable:
    description: Indicate if we don't want to enable USB2 HW LPM for host
      mode.
    type: boolean

  snps,usb3_lpm_capable:
    description: Determines if platform is USB3 LPM capable
    type: boolean

  snps,usb2-gadget-lpm-disable:
    description: Indicate if we don't want to enable USB2 HW LPM for gadget
      mode.
    type: boolean

  snps,reserved-endpoints:
    description:
      Reserve endpoints for other needs, e.g, for tracing control and output.
      When set, the driver will avoid using them for the regular USB transfers.
    $ref: /schemas/types.yaml#/definitions/uint8-array
    minItems: 1
    maxItems: 30
    items:
      minimum: 2
      maximum: 31

  snps,dis-start-transfer-quirk:
    description:
      When set, disable isoc START TRANSFER command failure SW work-around
      for DWC_usb31 version 1.70a-ea06 and prior.
    type: boolean

  snps,disable_scramble_quirk:
    description:
      True when SW should disable data scrambling. Only really useful for FPGA
      builds.
    type: boolean

  snps,has-lpm-erratum:
    description: True when DWC3 was configured with LPM Erratum enabled
    type: boolean

  snps,lpm-nyet-threshold:
    description: LPM NYET threshold
    $ref: /schemas/types.yaml#/definitions/uint8

  snps,u2exit_lfps_quirk:
    description: Set if we want to enable u2exit lfps quirk
    type: boolean

  snps,u2ss_inp3_quirk:
    description: Set if we enable P3 OK for U2/SS Inactive quirk
    type: boolean

  snps,req_p1p2p3_quirk:
    description:
      When set, the core will always request for P1/P2/P3 transition sequence.
    type: boolean

  snps,del_p1p2p3_quirk:
    description:
      When set core will delay P1/P2/P3 until a certain amount of 8B10B errors
      occur.
    type: boolean

  snps,del_phy_power_chg_quirk:
    description: When set core will delay PHY power change from P0 to P1/P2/P3.
    type: boolean

  snps,lfps_filter_quirk:
    description: When set core will filter LFPS reception.
    type: boolean

  snps,rx_detect_poll_quirk:
    description:
      when set core will disable a 400us delay to start Polling LFPS after
      RX.Detect.
    type: boolean

  snps,tx_de_emphasis_quirk:
    description: When set core will set Tx de-emphasis value
    type: boolean

  snps,tx_de_emphasis:
    description:
      The value driven to the PHY is controlled by the LTSSM during USB3
      Compliance mode.
    $ref: /schemas/types.yaml#/definitions/uint8
    enum:
      - 0 # -6dB de-emphasis
      - 1 # -3.5dB de-emphasis
      - 2 # No de-emphasis

  snps,dis_u3_susphy_quirk:
    description: When set core will disable USB3 suspend phy
    type: boolean

  snps,dis_u2_susphy_quirk:
    description: When set core will disable USB2 suspend phy
    type: boolean

  snps,dis_enblslpm_quirk:
    description:
      When set clears the enblslpm in GUSB2PHYCFG, disabling the suspend signal
      to the PHY.
    type: boolean

  snps,dis-u1-entry-quirk:
    description: Set if link entering into U1 needs to be disabled
    type: boolean

  snps,dis-u2-entry-quirk:
    description: Set if link entering into U2 needs to be disabled
    type: boolean

  snps,dis_rxdet_inp3_quirk:
    description:
      When set core will disable receiver detection in PHY P3 power state.
    type: boolean

  snps,dis-u2-freeclk-exists-quirk:
    description:
      When set, clear the u2_freeclk_exists in GUSB2PHYCFG, specify that USB2
      PHY doesn't provide a free-running PHY clock.
    type: boolean

  snps,dis-del-phy-power-chg-quirk:
    description:
      When set core will change PHY power from P0 to P1/P2/P3 without delay.
    type: boolean

  snps,dis-tx-ipgap-linecheck-quirk:
    description: When set, disable u2mac linestate check during HS transmit
    type: boolean

  snps,parkmode-disable-ss-quirk:
    description:
      When set, all SuperSpeed bus instances in park mode are disabled.
    type: boolean

  snps,parkmode-disable-hs-quirk:
    description:
      When set, all HighSpeed bus instances in park mode are disabled.
    type: boolean

  snps,dis_metastability_quirk:
    description:
      When set, disable metastability workaround. CAUTION! Use only if you are
      absolutely sure of it.
    type: boolean

  snps,dis-split-quirk:
    description:
      When set, change the way URBs are handled by the driver. Needed to
      avoid -EPROTO errors with usbhid on some devices (Hikey 970).
    type: boolean

  snps,gfladj-refclk-lpm-sel-quirk:
    description:
      When set, run the SOF/ITP counter based on ref_clk.
    type: boolean

  snps,resume-hs-terminations:
    description:
      Fix the issue of HS terminations CRC error on resume by enabling this
      quirk. When set, all the termsel, xcvrsel, opmode becomes 0 during end
      of resume. This option is to support certain legacy ULPI PHYs.
    type: boolean

  snps,ulpi-ext-vbus-drv:
    description:
      Some ULPI USB PHY does not support internal VBUS supply, and driving
      the CPEN pin, requires the configuration of the ulpi DRVVBUSEXTERNAL
      bit. When set, the xhci host will configure the USB2 PHY drives VBUS
      with an external supply.
    type: boolean

  snps,is-utmi-l1-suspend:
    description:
      True when DWC3 asserts output signal utmi_l1_suspend_n, false when
      asserts utmi_sleep_n.
    type: boolean

  snps,hird-threshold:
    description: HIRD threshold
    $ref: /schemas/types.yaml#/definitions/uint8

  snps,hsphy_interface:
    description:
      High-Speed PHY interface selection between UTMI+ and ULPI when the
      DWC_USB3_HSPHY_INTERFACE has value 3.
    $ref: /schemas/types.yaml#/definitions/string
    enum: [utmi, ulpi]

  snps,quirk-frame-length-adjustment:
    description:
      Value for GFLADJ_30MHZ field of GFLADJ register for post-silicon frame
      length adjustment when the fladj_30mhz_sdbnd signal is invalid or
      incorrect.
    $ref: /schemas/types.yaml#/definitions/uint32
    minimum: 0
    maximum: 0x3f

  snps,ref-clock-period-ns:
    description:
      Value for REFCLKPER field of GUCTL register for reference clock period in
      nanoseconds, when the hardware set default does not match the actual
      clock.

      This binding is deprecated. Instead, provide an appropriate reference clock.
    minimum: 8
    maximum: 62
    deprecated: true

  snps,rx-thr-num-pkt:
    description:
      USB RX packet threshold count. In host mode, this field specifies
      the space that must be available in the RX FIFO before the core can
      start the corresponding USB RX transaction (burst).
      In device mode, this field specifies the space that must be
      available in the RX FIFO before the core can send ERDY for a
      flow-controlled endpoint. It is only used for SuperSpeed.
      The valid values for this field are from 1 to 15. (DWC3 SuperSpeed
      USB 3.0 Controller Databook)
    $ref: /schemas/types.yaml#/definitions/uint8
    minimum: 1
    maximum: 15

  snps,rx-max-burst:
    description:
      Max USB RX burst size. In host mode, this field specifies the
      Maximum Bulk IN burst the DWC_usb3 core can perform. When the system
      bus is slower than the USB, RX FIFO can overrun during a long burst.
      You can program a smaller value to this field to limit the RX burst
      size that the core can perform. It only applies to SS Bulk,
      Isochronous, and Interrupt IN endpoints in the host mode.
      In device mode, this field specifies the NUMP value that is sent in
      ERDY for an OUT endpoint.
      The valid values for this field are from 1 to 16. (DWC3 SuperSpeed
      USB 3.0 Controller Databook)
    $ref: /schemas/types.yaml#/definitions/uint8
    minimum: 1
    maximum: 16

  snps,tx-thr-num-pkt:
    description:
      USB TX packet threshold count. This field specifies the number of
      packets that must be in the TXFIFO before the core can start
      transmission for the corresponding USB transaction (burst).
      This count is valid in both host and device modes. It is only used
      for SuperSpeed operation.
      Valid values are from 1 to 15. (DWC3 SuperSpeed USB 3.0 Controller
      Databook)
    $ref: /schemas/types.yaml#/definitions/uint8
    minimum: 1
    maximum: 15

  snps,tx-max-burst:
    description:
      Max USB TX burst size. When the system bus is slower than the USB,
      TX FIFO can underrun during a long burst. Program a smaller value
      to this field to limit the TX burst size that the core can execute.
      In Host mode, it only applies to SS Bulk, Isochronous, and Interrupt
      OUT endpoints. This value is not used in device mode.
      Valid values are from 1 to 16. (DWC3 SuperSpeed USB 3.0 Controller
      Databook)
    $ref: /schemas/types.yaml#/definitions/uint8
    minimum: 1
    maximum: 16

  snps,rx-thr-num-pkt-prd:
    description:
      Periodic ESS RX packet threshold count (host mode only). Set this and
      snps,rx-max-burst-prd to a valid, non-zero value 1-16 (DWC_usb31
      programming guide section 1.2.4) to enable periodic ESS RX threshold.
    $ref: /schemas/types.yaml#/definitions/uint8
    minimum: 1
    maximum: 16

  snps,rx-max-burst-prd:
    description:
      Max periodic ESS RX burst size (host mode only). Set this and
      snps,rx-thr-num-pkt-prd to a valid, non-zero value 1-16 (DWC_usb31
      programming guide section 1.2.4) to enable periodic ESS RX threshold.
    $ref: /schemas/types.yaml#/definitions/uint8
    minimum: 1
    maximum: 16

  snps,tx-thr-num-pkt-prd:
    description:
      Periodic ESS TX packet threshold count (host mode only). Set this and
      snps,tx-max-burst-prd to a valid, non-zero value 1-16 (DWC_usb31
      programming guide section 1.2.3) to enable periodic ESS TX threshold.
    $ref: /schemas/types.yaml#/definitions/uint8
    minimum: 1
    maximum: 16

  snps,tx-max-burst-prd:
    description:
      Max periodic ESS TX burst size (host mode only). Set this and
      snps,tx-thr-num-pkt-prd to a valid, non-zero value 1-16 (DWC_usb31
      programming guide section 1.2.3) to enable periodic ESS TX threshold.
    $ref: /schemas/types.yaml#/definitions/uint8
    minimum: 1
    maximum: 16

  tx-fifo-resize:
    description: Determines if the TX fifos can be dynamically resized depending
      on the number of IN endpoints used and if bursting is supported.  This
      may help improve bandwidth on platforms with higher system latencies, as
      increased fifo space allows for the controller to prefetch data into its
      internal memory.
    type: boolean

  tx-fifo-max-num:
    description: Specifies the max number of packets the txfifo resizing logic
      can account for when higher endpoint bursting is used. (bMaxBurst > 6) The
      higher the number, the more fifo space the txfifo resizing logic will
      allocate for that endpoint.
    $ref: /schemas/types.yaml#/definitions/uint8
    minimum: 3

  snps,incr-burst-type-adjustment:
    description:
      Value for INCR burst type of GSBUSCFG0 register, undefined length INCR
      burst type enable and INCRx type. A single value means INCRX burst mode
      enabled. If more than one value specified, undefined length INCR burst
      type will be enabled with burst lengths utilized up to the maximum
      of the values passed in this property.
    $ref: /schemas/types.yaml#/definitions/uint32-array
    minItems: 1
    maxItems: 8
    uniqueItems: true
    items:
      enum: [1, 4, 8, 16, 32, 64, 128, 256]

  num-hc-interrupters:
    maximum: 8
    default: 1

  connector:
    $ref: /schemas/connector/usb-connector.yaml#
    description: Connector for dual role switch
    type: object
    unevaluatedProperties: false

  port:
    $ref: /schemas/graph.yaml#/properties/port
    description:
      This port is used with the 'usb-role-switch' property  to connect the
      dwc3 to type C connector.

  ports:
    $ref: /schemas/graph.yaml#/properties/ports
    description:
      Those ports should be used with any connector to the data bus of this
      controller using the OF graph bindings specified if the "usb-role-switch"
      property is used.

    properties:
      port@0:
        $ref: /schemas/graph.yaml#/properties/port
        description: High Speed (HS) data bus.

      port@1:
        $ref: /schemas/graph.yaml#/properties/port
        description: Super Speed (SS) data bus.

  wakeup-source:
    $ref: /schemas/types.yaml#/definitions/flag
    description:
      Enable USB remote wakeup.

required:
  - compatible
  - reg

additionalProperties: true
...

