# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
%YAML 1.2
---
$id: http://devicetree.org/schemas/usb/nvidia,tegra194-xusb.yaml#
$schema: http://devicetree.org/meta-schemas/core.yaml#

title: NVIDIA Tegra194 xHCI controller

maintainers:
  - Thierry Reding <thierry.reding@gmail.com>
  - Jon Hunter <jonathanh@nvidia.com>

description: The Tegra xHCI controller supports both USB2 and USB3 interfaces
  exposed by the Tegra XUSB pad controller.

properties:
  compatible:
    const: nvidia,tegra194-xusb

  reg:
    items:
      - description: base and length of the xHCI host registers
      - description: base and length of the XUSB FPCI registers

  reg-names:
    items:
      - const: hcd
      - const: fpci

  interrupts:
    items:
      - description: xHCI host interrupt
      - description: mailbox interrupt

  clocks:
    items:
      - description: XUSB host clock
      - description: XUSB Falcon source clock
      - description: XUSB SuperSpeed clock
      - description: XUSB SuperSpeed source clock
      - description: XUSB HighSpeed clock source
      - description: XUSB FullSpeed clock source
      - description: USB PLL
      - description: reference clock
      - description: I/O PLL

  clock-names:
    items:
      - const: xusb_host
      - const: xusb_falcon_src
      - const: xusb_ss
      - const: xusb_ss_src
      - const: xusb_hs_src
      - const: xusb_fs_src
      - const: pll_u_480m
      - const: clk_m
      - const: pll_e

  interconnects:
    items:
      - description: read client
      - description: write client

  interconnect-names:
    items:
      - const: dma-mem # read
      - const: write

  iommus:
    maxItems: 1

  nvidia,xusb-padctl:
    $ref: /schemas/types.yaml#/definitions/phandle
    description: phandle to the XUSB pad controller that is used to configure
      the USB pads used by the XHCI controller

  phys:
    minItems: 1
    maxItems: 8

  phy-names:
    minItems: 1
    maxItems: 8
    items:
      enum:
        - usb2-0
        - usb2-1
        - usb2-2
        - usb2-3
        - usb3-0
        - usb3-1
        - usb3-2
        - usb3-3

  power-domains:
    items:
      - description: XUSBC power domain (for Host and USB 2.0)
      - description: XUSBA power domain (for SuperSpeed)

  power-domain-names:
    items:
      - const: xusb_host
      - const: xusb_ss

  dvddio-pex-supply:
    description: PCIe/USB3 analog logic power supply. Must supply 1.05 V.

  hvddio-pex-supply:
    description: High-voltage PCIe/USB3 power supply. Must supply 1.8 V.

  avdd-usb-supply:
    description: USB controller power supply. Must supply 3.3 V.

  avdd-pll-utmip-supply:
    description: UTMI PLL power supply. Must supply 1.8 V.

  avdd-pll-uerefe-supply:
    description: PLLE reference PLL power supply. Must supply 1.05 V.

  dvdd-usb-ss-pll-supply:
    description: PCIe/USB3 PLL power supply. Must supply 1.05 V.

  hvdd-usb-ss-pll-e-supply:
    description: High-voltage PLLE power supply. Must supply 1.8 V.

allOf:
  - $ref: usb-xhci.yaml

unevaluatedProperties: false

examples:
  - |
    #include <dt-bindings/clock/tegra194-clock.h>
    #include <dt-bindings/interrupt-controller/arm-gic.h>
    #include <dt-bindings/memory/tegra194-mc.h>
    #include <dt-bindings/power/tegra194-powergate.h>
    #include <dt-bindings/reset/tegra194-reset.h>

    usb@3610000 {
        compatible = "nvidia,tegra194-xusb";
        reg = <0x03610000 0x40000>,
              <0x03600000 0x10000>;
        reg-names = "hcd", "fpci";

        interrupts = <GIC_SPI 163 IRQ_TYPE_LEVEL_HIGH>,
                     <GIC_SPI 164 IRQ_TYPE_LEVEL_HIGH>;

        clocks = <&bpmp TEGRA194_CLK_XUSB_CORE_HOST>,
                 <&bpmp TEGRA194_CLK_XUSB_FALCON>,
                 <&bpmp TEGRA194_CLK_XUSB_CORE_SS>,
                 <&bpmp TEGRA194_CLK_XUSB_SS>,
                 <&bpmp TEGRA194_CLK_CLK_M>,
                 <&bpmp TEGRA194_CLK_XUSB_FS>,
                 <&bpmp TEGRA194_CLK_UTMIPLL>,
                 <&bpmp TEGRA194_CLK_CLK_M>,
                 <&bpmp TEGRA194_CLK_PLLE>;
        clock-names = "xusb_host", "xusb_falcon_src",
                      "xusb_ss", "xusb_ss_src", "xusb_hs_src",
                      "xusb_fs_src", "pll_u_480m", "clk_m",
                      "pll_e";
        interconnects = <&mc TEGRA194_MEMORY_CLIENT_XUSB_HOSTR &emc>,
                        <&mc TEGRA194_MEMORY_CLIENT_XUSB_HOSTW &emc>;
        interconnect-names = "dma-mem", "write";
        iommus = <&smmu TEGRA194_SID_XUSB_HOST>;

        power-domains = <&bpmp TEGRA194_POWER_DOMAIN_XUSBC>,
                        <&bpmp TEGRA194_POWER_DOMAIN_XUSBA>;
        power-domain-names = "xusb_host", "xusb_ss";

        nvidia,xusb-padctl = <&xusb_padctl>;

        phys = <&phy_usb2_0>, <&phy_usb2_1>, <&phy_usb2_3>, <&phy_usb3_0>,
               <&phy_usb3_2>, <&phy_usb3_3>;
        phy-names = "usb2-0", "usb2-1", "usb2-3", "usb3-0", "usb3-2", "usb3-3";
    };
