# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
%YAML 1.2
---
$id: http://devicetree.org/schemas/w1/maxim,ds2482.yaml#
$schema: http://devicetree.org/meta-schemas/core.yaml#

title: Maxim One wire bus master controller

maintainers:
  - Stefan Wahren <stefan.wahren@chargebyte.com>

description: |
  I2C to 1-wire bridges

  https://www.analog.com/media/en/technical-documentation/data-sheets/ds2482-100.pdf
  https://www.analog.com/media/en/technical-documentation/data-sheets/DS2482-800.pdf
  https://www.analog.com/media/en/technical-documentation/data-sheets/DS2484.pdf

properties:
  compatible:
    enum:
      - maxim,ds2482
      - maxim,ds2484

  reg:
    maxItems: 1

  vcc-supply: true

required:
  - compatible
  - reg

additionalProperties:
  type: object

examples:
  - |
    i2c {
      #address-cells = <1>;
      #size-cells = <0>;
      onewire@18 {
        compatible = "maxim,ds2484";
        reg = <0x18>;
      };
    };
