# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
%YAML 1.2
---
$id: http://devicetree.org/schemas/thermal/fsl,scu-thermal.yaml#
$schema: http://devicetree.org/meta-schemas/core.yaml#

title: i.MX SCU Client Device Node - Thermal Based on SCU Message Protocol

maintainers:
  - Dong Aisheng <aisheng.dong@nxp.com>

description: i.MX SCU Client Device Node
  Client nodes are maintained as children of the relevant IMX-SCU device node.

allOf:
  - $ref: thermal-sensor.yaml#

properties:
  compatible:
    items:
      - enum:
          - fsl,imx8dxl-sc-thermal
          - fsl,imx8qxp-sc-thermal
      - const: fsl,imx-sc-thermal

  '#thermal-sensor-cells':
    const: 1

required:
  - compatible

additionalProperties: false

examples:
  - |
    thermal-sensor {
        compatible = "fsl,imx8qxp-sc-thermal", "fsl,imx-sc-thermal";
        #thermal-sensor-cells = <1>;
    };
