.. SPDX-License-Identifier: GPL-2.0

Kernel driver adp1050
=====================

Supported chips:

  * Analog Devices ADP1050

    Prefix: 'adp1050'

    Addresses scanned: I2C 0x70 - 0x77

    Datasheet: https://www.analog.com/media/en/technical-documentation/data-sheets/ADP1050.pdf

  * Analog Devices ADP1051

    Prefix: 'adp1051'

    Addresses scanned: I2C 0x70 - 0x77

    Datasheet: https://www.analog.com/media/en/technical-documentation/data-sheets/ADP1051.pdf

  * Analog Devices ADP1055

    Prefix: 'adp1055'

    Addresses scanned: I2C 0x4B - 0x77

    Datasheet: https://www.analog.com/media/en/technical-documentation/data-sheets/ADP1055.pdf

  * Analog Devices LTP8800-1A/-2/-4A

    Prefix: 'ltp8800'

    Addresses scanned: -

    Datasheet: https://www.analog.com/media/en/technical-documentation/data-sheets/LTP8800-1A.pdf
         https://www.analog.com/media/en/technical-documentation/data-sheets/LTP8800-2.pdf
         https://www.analog.com/media/en/technical-documentation/data-sheets/LTP8800-4A.pdf

Authors:

  - Radu Sabau <radu.sabau@analog.com>


Description
-----------

This driver supports hardware monitoring for Analog Devices ADP1050, ADP1051,
and ADP1055 Digital Controller for Isolated Power Supply with PMBus interface,
and the LTP8800 step-down μModule regulators.

The ADP1050, ADP1051, and ADP1055 are advanced digital controllers with PMBus™
interface targeting high density, high efficiency dc-to-dc power
conversion used to monitor system temperatures, voltages and currents. The
LTP8800 is a family of step-down μModule regulators that provides microprocessor
core voltage from 54V power distribution architecture. Through the PMBus
interface, the device can monitor input/output voltages, input current and
temperature.

Usage Notes
-----------

This driver does not auto-detect devices. You will have to instantiate
the devices explicitly.
Please see Documentation/i2c/instantiating-devices.rst for details.

Platform data support
---------------------

The driver supports standard PMBus driver platform data.

Sysfs Attributes
----------------

================= ========================================
in1_label         "vin"
in1_input         Measured input voltage
in1_alarm	  Input voltage alarm
in1_crit          Critical maximum input voltage
in1_crit_alarm    Input voltage high alarm
in1_lcrit         Critical minimum input voltage
in1_lcrit_alarm   Input voltage critical low alarm
in2_label	  "vout1"
in2_input	  Measured output voltage
in2_crit	  Critical maximum output voltage
in2_crit_alarm    Output voltage high alarm
in2_lcrit	  Critical minimum output voltage
in2_lcrit_alarm	  Output voltage critical low alarm
in2_max           Critical maximum output voltage
in2_max_alarm     Output voltage critical max alarm
in2_min           Critical minimum output voltage
in2_min_alarm     Output voltage critical min alarm
curr1_label	  "iin"
curr1_input	  Measured input current.
curr1_alarm	  Input current alarm
curr1_crit        Critical maximum input current
curr1_crit_alarm  Input current high alarm
curr2_label       "iout1"
curr2_input       Measured output current
curr2_alarm	  Output current alarm
curr2_crit        Critical maximum output current
curr2_crit_alarm  Output current high alarm
curr2_lcrit       Critical minimum output current
curr2_lcrit_alarm Output current critical low alarm
curr2_max         Critical maximum output current
curr2_max_alarm   Output current critical max alarm
power1_label      "pout1"
power1_input      Measured output power
power1_crit       Critical maximum output power
power1_crit_alarm Output power high alarm
temp1_input       Measured temperature
temp1_crit	  Critical high temperature
temp1_crit_alarm  Chip temperature critical high alarm
temp1_max         Critical maximum temperature
temp1_max_alarm   Temperature critical max alarm
temp2_input       Measured temperature
temp2_crit        Critical high temperature
temp2_crit_alarm  Chip temperature critical high alarm
temp2_max         Critical maximum temperature
temp2_max_alarm   Temperature critical max alarm
================= ========================================
