Owner Module/Drivers,Group,Property Name,Type,Property Values,Object attached,Description/Restrictions
,DVI-I,“subconnector”,ENUM,"{ “Unknown”, “DVI-D”, “DVI-A” }",Connector,TBD
,,“select subconnector”,ENUM,"{ “Automatic”, “DVI-D”, “DVI-A” }",Connector,TBD
,TV,“subconnector”,ENUM,"{ ""Unknown"", ""Composite"", ""SVIDEO"", ""Component"", ""SCART"" }",Connector,TBD
,,“select subconnector”,ENUM,"{ ""Automatic"", ""Composite"", ""SVIDEO"", ""Component"", ""SCART"" }",Connector,TBD
,,“mode”,ENUM,"{ ""NTSC_M"", ""NTSC_J"", ""NTSC_443"", ""PAL_B"" } etc.",Connector,TBD
,,“left margin”,RANGE,"Min=0, Max=100",Connector,TBD
,,“right margin”,RANGE,"Min=0, Max=100",Connector,TBD
,,“top margin”,RANGE,"Min=0, Max=100",Connector,TBD
,,“bottom margin”,RANGE,"Min=0, Max=100",Connector,TBD
,,“brightness”,RANGE,"Min=0, Max=100",Connector,TBD
,,“contrast”,RANGE,"Min=0, Max=100",Connector,TBD
,,“flicker reduction”,RANGE,"Min=0, Max=100",Connector,TBD
,,“overscan”,RANGE,"Min=0, Max=100",Connector,TBD
,,“saturation”,RANGE,"Min=0, Max=100",Connector,TBD
,,“hue”,RANGE,"Min=0, Max=100",Connector,TBD
,Virtual GPU,“suggested X”,RANGE,"Min=0, Max=0xffffffff",Connector,property to suggest an X offset for a connector
,,“suggested Y”,RANGE,"Min=0, Max=0xffffffff",Connector,property to suggest an Y offset for a connector
,Optional,"""aspect ratio""",ENUM,"{ ""None"", ""4:3"", ""16:9"" }",Connector,TDB
,,“audio”,ENUM,"{ ""force-dvi"", ""off"", ""auto"", ""on"" }",Connector,TBD
,SDVO-TV,“mode”,ENUM,"{ ""NTSC_M"", ""NTSC_J"", ""NTSC_443"", ""PAL_B"" } etc.",Connector,TBD
,,"""left_margin""",RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,"""right_margin""",RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,"""top_margin""",RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,"""bottom_margin""",RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“hpos”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“vpos”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“contrast”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“saturation”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“hue”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“sharpness”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“flicker_filter”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“flicker_filter_adaptive”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“flicker_filter_2d”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“tv_chroma_filter”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“tv_luma_filter”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“dot_crawl”,RANGE,"Min=0, Max=1",Connector,TBD
,SDVO-TV/LVDS,“brightness”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
CDV gma-500,Generic,"""Broadcast RGB""",ENUM,"{ “Full”, “Limited 16:235” }",Connector,TBD
Poulsbo,Generic,“backlight”,RANGE,"Min=0, Max=100",Connector,TBD
,SDVO-TV,“mode”,ENUM,"{ ""NTSC_M"", ""NTSC_J"", ""NTSC_443"", ""PAL_B"" } etc.",Connector,TBD
,,"""left_margin""",RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,"""right_margin""",RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,"""top_margin""",RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,"""bottom_margin""",RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“hpos”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“vpos”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“contrast”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“saturation”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“hue”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“sharpness”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“flicker_filter”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“flicker_filter_adaptive”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“flicker_filter_2d”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“tv_chroma_filter”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“tv_luma_filter”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
,,“dot_crawl”,RANGE,"Min=0, Max=1",Connector,TBD
,SDVO-TV/LVDS,“brightness”,RANGE,"Min=0, Max= SDVO dependent",Connector,TBD
armada,CRTC,"""CSC_YUV""",ENUM,"{ ""Auto"" , ""CCIR601"", ""CCIR709"" }",CRTC,TBD
,,"""CSC_RGB""",ENUM,"{ ""Auto"", ""Computer system"", ""Studio"" }",CRTC,TBD
,Overlay,"""colorkey""",RANGE,"Min=0, Max=0xffffff",Plane,TBD
,,"""colorkey_min""",RANGE,"Min=0, Max=0xffffff",Plane,TBD
,,"""colorkey_max""",RANGE,"Min=0, Max=0xffffff",Plane,TBD
,,"""colorkey_val""",RANGE,"Min=0, Max=0xffffff",Plane,TBD
,,"""colorkey_alpha""",RANGE,"Min=0, Max=0xffffff",Plane,TBD
,,"""colorkey_mode""",ENUM,"{ ""disabled"", ""Y component"", ""U component"" , ""V component"", ""RGB"", “R component"", ""G component"", ""B component"" }",Plane,TBD
,,"""brightness""",RANGE,"Min=0, Max=256 + 255",Plane,TBD
,,"""contrast""",RANGE,"Min=0, Max=0x7fff",Plane,TBD
,,"""saturation""",RANGE,"Min=0, Max=0x7fff",Plane,TBD
exynos,CRTC,“mode”,ENUM,"{ ""normal"", ""blank"" }",CRTC,TBD
i2c/ch7006_drv,Generic,“scale”,RANGE,"Min=0, Max=2",Connector,TBD
,TV,“mode”,ENUM,"{ ""PAL"", ""PAL-M"",""PAL-N""}, ”PAL-Nc"" , ""PAL-60"", ""NTSC-M"", ""NTSC-J"" }",Connector,TBD
nouveau,NV10 Overlay,"""colorkey""",RANGE,"Min=0, Max=0x01ffffff",Plane,TBD
,,“contrast”,RANGE,"Min=0, Max=8192-1",Plane,TBD
,,“brightness”,RANGE,"Min=0, Max=1024",Plane,TBD
,,“hue”,RANGE,"Min=0, Max=359",Plane,TBD
,,“saturation”,RANGE,"Min=0, Max=8192-1",Plane,TBD
,,“iturbt_709”,RANGE,"Min=0, Max=1",Plane,TBD
,Nv04 Overlay,“colorkey”,RANGE,"Min=0, Max=0x01ffffff",Plane,TBD
,,“brightness”,RANGE,"Min=0, Max=1024",Plane,TBD
,Display,“dithering mode”,ENUM,"{ ""auto"", ""off"", ""on"" }",Connector,TBD
,,“dithering depth”,ENUM,"{ ""auto"", ""off"", ""on"", ""static 2x2"", ""dynamic 2x2"", ""temporal"" }",Connector,TBD
,,“underscan”,ENUM,"{ ""auto"", ""6 bpc"", ""8 bpc"" }",Connector,TBD
,,“underscan hborder”,RANGE,"Min=0, Max=128",Connector,TBD
,,“underscan vborder”,RANGE,"Min=0, Max=128",Connector,TBD
,,“vibrant hue”,RANGE,"Min=0, Max=180",Connector,TBD
,,“color vibrance”,RANGE,"Min=0, Max=200",Connector,TBD
omap,Generic,“zorder”,RANGE,"Min=0, Max=3","CRTC, Plane",TBD
qxl,Generic,"“hotplug_mode_update""",RANGE,"Min=0, Max=1",Connector,TBD
radeon,DVI-I,“coherent”,RANGE,"Min=0, Max=1",Connector,TBD
,DAC enable load detect,“load detection”,RANGE,"Min=0, Max=1",Connector,TBD
,TV Standard,"""tv standard""",ENUM,"{ ""ntsc"", ""pal"", ""pal-m"", ""pal-60"", ""ntsc-j"" , ""scart-pal"", ""pal-cn"", ""secam"" }",Connector,TBD
,legacy TMDS PLL detect,"""tmds_pll""",ENUM,"{ ""driver"", ""bios"" }",-,TBD
,Underscan,"""underscan""",ENUM,"{ ""off"", ""on"", ""auto"" }",Connector,TBD
,,"""underscan hborder""",RANGE,"Min=0, Max=128",Connector,TBD
,,"""underscan vborder""",RANGE,"Min=0, Max=128",Connector,TBD
,Audio,“audio”,ENUM,"{ ""off"", ""on"", ""auto"" }",Connector,TBD
,FMT Dithering,“dither”,ENUM,"{ ""off"", ""on"" }",Connector,TBD
,,"""colorkey""",RANGE,"Min=0, Max=0x01ffffff",Plane,TBD
