| # UMAX Mirage scanners

Index Frontend options: Standard options Advanced options Supported scanners: Power Look series Mirage series Astra series Vista series UC series others Not listed scanners UMAX scanner clones UMAX parallel port scanners Configuration Speed of UMAX scanners SANE-umax homepage SANE homepage XSane homepage |
UMAX scanners
Mirage series:
Name | SCSI-ID | Versions | UTA | ADF | B/W | Gray | Color | Bits/pixel | Resolution
Mirage | Mirage D-16L | all (2.7) | incl |  | ok | ok | ok | 1,8,10,24,30 | 400 x 800 800 x 1600*
Mirage II | Mirage II | all (1.6) | incl |  | ok | ok | ok | 1,8,12,24,36 | 700 x 1400 1400 x 2800
Mirage IIse | Mirage IIse | ? | incl |  | ? | ? | ? | 1,8,12,24,36 | 700 x 1400
* Mirage D-16L scanners allow scanning up to 800x800 / 1600x1600 dpi. UTA = Umax Transparency Adapter, ADF = Automatic Document Feeder (X = supported by scanner, incl = is included) This page has been changed on 12th. february 2001

> Author: Oliver Rauch