| # UMAX scanner clones

Index Frontend options: Standard options Advanced options Supported scanners: Power Look series Mirage series Astra series Vista series UC series others Not listed scanners UMAX scanner clones UMAX parallel port scanners Configuration Speed of UMAX scanners SANE-umax homepage SANE homepage XSane homepage | The sane-umax library implements a SANE backend that provides access to several scanners that are compatible to the UMAX-SCSI-protocoll! Here is a list of the UMAX-compatible scanners:
UMAX compatible Linotype Hell scanners
Name | Vendor | SCSI-ID | Versions | UTA | ADF | B/W | Grays | Color | Bits/pixel | Resolution
Jade | LinoHell | Office | all | X | X | ok | ok | ok | 1,8,24 | 600 x 1200*
Jade | LinoHell | JADE | all | X | X | ok | ok | ok | 1,8,24 | 600 x 1200*
Jade2 | LinoHell | Office2 | all | X |  | ok | ok | ok | 1,8,10,24,30 | 600 x 1200
Saphir | LinoHell | unknown |  | incl |  |  |  |  | 1,8,10,24,30 | 600 x 1200
Saphir2 | LinoHell | SAPHIR2 | all | incl |  | ok | ok | ok | 1,8,12,24,36 | 600 x 1200
Saphir Ultra | LinoHell | unknown |  | incl |  |  |  |  | 1,8,12,24,36 | 600 x 1200
Saphir Ultra II | LinoHell | unknown |  | incl |  |  |  |  | 1,8,14,24,42 | 1200 x 2400
Saphir HiRes | LinoHell | unknown |  | incl |  |  |  |  | 1,8,14,24,42 | 1220 x 3048 3048 x 3048
Opal | LinoHell | unknown |  | incl |  |  |  |  | 1,8,10,24,30 | 700 x 1400
Opal2 | LinoHell | OPAL2 |  | incl |  | ok | ok | ok | 1,8,12,24,36 | 700 x 1400
Opal Ultra | LinoHell | unknown |  | incl |  |  |  |  | 1,8,12,24,36 | 700 x 1400 1400 x 2800
Linoscan 1400 | HDM | LS4H1S | ? | X |  | ok | ok | ok | 1,8,12,14,24,36,42 | 1200 x 2400
* Scanner is able to scan up to 1200 x 1200 dpi. UTA = Umax Transparency Adapter, ADF = Automatic Document Feeder (X = supported by scanner, incl = is included)
Other UMAX compatible scanners
Name | Vendor | SCSI-ID | Versions | UTA | ADF | B/W | Gray | Color | Bits/pixel | Resolution
Vobis/Highscreen Scanboostar Premium | LinoHell | Office2 | all | X |  | ok | ok | ok | 1,8,10,24,30 | 600 x 1200
Escom Image Scanner 256 | UMAX | UG80 | all | -- |  | ok | ok | -- | 1,8 | 300 x 300
Nikon AX-210 | Nikon | AX-210 | all(?) | X | X | ok | ok | ok | 1,8,24 | 600 x 1200*
Genius Colorpage HR5 (normal and Pro) | KYE | ColorPage-HR5 | all(?) | X |  | ok | ok | ok | 1,8,10,24,30 | 600 x 1200
Epson Perfection 600 | EPSON | Perfection600 | all(2.3) | X |  | ok | ok | ok | 1,8,10,24,30 | 600 x 1200
Escort Galleria 600S | ESCORT | Galleria 600S | all(1.6) | X |  | ?? | ?? | ?? | 1,8,24 | 300 x 600
* Scanner is able to scan up to 1200 x 1200 dpi. UTA = Umax Transparency Adapter, ADF = Automatic Document Feeder (X = supported by scanner, incl = is included) This page has been changed on 1st. october 2004

> Author: Oliver Rauch