liblzma (XZ Utils) 5.8.1

Data Structures | Macros | Functions
bcj.h File Reference

Branch/Call/Jump conversion filters. More...

## Data Structures
struct | lzma_options_bcj
| Options for BCJ filters. More...

## Macros
#define | LZMA_FILTER_X86 LZMA_VLI_C(0x04)
| Filter for x86 binaries.
#define | LZMA_FILTER_POWERPC LZMA_VLI_C(0x05)
| Filter for Big endian PowerPC binaries.
#define | LZMA_FILTER_IA64 LZMA_VLI_C(0x06)
| Filter for IA-64 (Itanium) binaries.
#define | LZMA_FILTER_ARM LZMA_VLI_C(0x07)
| Filter for ARM binaries.
#define | LZMA_FILTER_ARMTHUMB LZMA_VLI_C(0x08)
| Filter for ARM-Thumb binaries.
#define | LZMA_FILTER_SPARC LZMA_VLI_C(0x09)
| Filter for SPARC binaries.
#define | LZMA_FILTER_ARM64 LZMA_VLI_C(0x0A)
| Filter for ARM64 binaries.
#define | LZMA_FILTER_RISCV LZMA_VLI_C(0x0B)
| Filter for RISC-V binaries.

## Functions
size_t | lzma_bcj_arm64_encode (uint32_t start_offset, uint8_t *buf, size_t size) lzma_nothrow
| Raw ARM64 BCJ encoder.
size_t | lzma_bcj_arm64_decode (uint32_t start_offset, uint8_t *buf, size_t size) lzma_nothrow
| Raw ARM64 BCJ decoder.
size_t | lzma_bcj_riscv_encode (uint32_t start_offset, uint8_t *buf, size_t size) lzma_nothrow
| Raw RISC-V BCJ encoder.
size_t | lzma_bcj_riscv_decode (uint32_t start_offset, uint8_t *buf, size_t size) lzma_nothrow
| Raw RISC-V BCJ decoder.
size_t | lzma_bcj_x86_encode (uint32_t start_offset, uint8_t *buf, size_t size) lzma_nothrow
| Raw x86 BCJ encoder.
size_t | lzma_bcj_x86_decode (uint32_t start_offset, uint8_t *buf, size_t size) lzma_nothrow
| Raw x86 BCJ decoder.

## Detailed Description

Branch/Call/Jump conversion filters.

Note
  Never include this file directly. Use <lzma.h> instead.

## Function Documentation

## ◆ lzma_bcj_arm64_encode()

size_t lzma_bcj_arm64_encode | ( | uint32_t | start_offset,
|  | uint8_t * | buf,
|  | size_t | size )
| extern

Raw ARM64 BCJ encoder.

This is for special use cases only.

Parameters

  start_offset | The lowest 32 bits of the offset in the executable being filtered. For the ARM64 filter, this must be a multiple of four. For the very best results, this should also be in sync with 4096-byte page boundaries in the executable due to how ARM64's ADRP instruction works.
  buf | Buffer to be filtered in place
  size | Size of the buffer

Returns
  Number of bytes that were processed in `buf`. This is at most `size`. With the ARM64 filter, the return value is always a multiple of 4, and at most 3 bytes are left unfiltered.

Since
  5.7.1alpha

## ◆ lzma_bcj_arm64_decode()

size_t lzma_bcj_arm64_decode | ( | uint32_t | start_offset,
|  | uint8_t * | buf,
|  | size_t | size )
| extern

Raw ARM64 BCJ decoder.

See lzma_bcj_arm64_encode().

Since
  5.7.1alpha

## ◆ lzma_bcj_riscv_encode()

size_t lzma_bcj_riscv_encode | ( | uint32_t | start_offset,
|  | uint8_t * | buf,
|  | size_t | size )
| extern

Raw RISC-V BCJ encoder.

This is for special use cases only.

Parameters

  start_offset | The lowest 32 bits of the offset in the executable being filtered. For the RISC-V filter, this must be a multiple of 2.
  buf | Buffer to be filtered in place
  size | Size of the buffer

Returns
  Number of bytes that were processed in `buf`. This is at most `size`. With the RISC-V filter, the return value is always a multiple of 2, and at most 7 bytes are left unfiltered.

Since
  5.7.1alpha

## ◆ lzma_bcj_riscv_decode()

size_t lzma_bcj_riscv_decode | ( | uint32_t | start_offset,
|  | uint8_t * | buf,
|  | size_t | size )
| extern

Raw RISC-V BCJ decoder.

See lzma_bcj_riscv_encode().

Since
  5.7.1alpha

## ◆ lzma_bcj_x86_encode()

size_t lzma_bcj_x86_encode | ( | uint32_t | start_offset,
|  | uint8_t * | buf,
|  | size_t | size )
| extern

Raw x86 BCJ encoder.

This is for special use cases only.

Parameters

  start_offset | The lowest 32 bits of the offset in the executable being filtered. For the x86 filter, all values are valid.
  buf | Buffer to be filtered in place
  size | Size of the buffer

Returns
  Number of bytes that were processed in `buf`. This is at most `size`. For the x86 filter, the return value is always a multiple of 1, and at most 4 bytes are left unfiltered.

Since
  5.7.1alpha

## ◆ lzma_bcj_x86_decode()

size_t lzma_bcj_x86_decode | ( | uint32_t | start_offset,
|  | uint8_t * | buf,
|  | size_t | size )
| extern

Raw x86 BCJ decoder.

See lzma_bcj_x86_encode().

Since
  5.7.1alpha