# Function _mm512_mask_i32gather_ps

1.89.0 · Source

    pub unsafe fn _mm512_mask_i32gather_ps(
        src: __m512,
        mask: __mmask16,
        offsets: __m512i,
        slice: *const f32,
        const SCALE: i32,
    ) -> __m512

Available on (x86 or x86-64) and target feature `avx512f` and x86-64 only.
Expand description

Gather single-precision (32-bit) floating-point elements from memory using 32-bit indices. 32-bit elements are loaded from addresses starting at base_addr and offset by each 32-bit element in vindex (each index is scaled by the factor in scale). Gathered elements are merged into dst using writemask k (elements are copied from src when the corresponding mask bit is not set). scale should be 1, 2, 4 or 8.

Intel’s documentation