# Function _mm512_permutex2var_ps

1.89.0 · Source

    pub fn _mm512_permutex2var_ps(a: __m512, idx: __m512i, b: __m512) -> __m512

Available on (x86 or x86-64) and target feature `avx512f` and x86-64 only.
Expand description

Shuffle single-precision (32-bit) floating-point elements in a and b across lanes using the corresponding selector and index in idx, and store the results in dst.

Intel’s documentation