# Function _mm512_fixupimm_ps

1.89.0 · Source

    pub fn _mm512_fixupimm_ps(
        a: __m512,
        b: __m512,
        c: __m512i,
        const IMM8: i32,
    ) -> __m512

Available on (x86 or x86-64) and target feature `avx512f` and x86 only.
Expand description

Fix up packed single-precision (32-bit) floating-point elements in a and b using packed 32-bit integers in c, and store the results in dst. imm8 is used to set the required flags reporting.

Intel’s documentation