# Function _mm512_maskz_min_ps

1.89.0 · Source

    pub fn _mm512_maskz_min_ps(k: __mmask16, a: __m512, b: __m512) -> __m512

Available on (x86 or x86-64) and target feature `avx512f` and x86 only.
Expand description

Compare packed single-precision (32-bit) floating-point elements in a and b, and store packed minimum values in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation