# Function _mm_cmplt_ps

1.27.0 · Source

    pub fn _mm_cmplt_ps(a: __m128, b: __m128) -> __m128

Available on (x86 or x86-64) and target feature `sse` and x86 only.
Expand description

Compares each of the four floats in `a` to the corresponding element in `b`. The result in the output vector will be `0xffffffff` if the input element in `a` is less than the corresponding element in `b`, or `0` otherwise.

Intel’s documentation