# Function _mm_setr_ps

1.27.0 · Source

    pub fn _mm_setr_ps(a: f32, b: f32, c: f32, d: f32) -> __m128

Available on (x86 or x86-64) and target feature `sse` and x86 only.
Expand description

Construct a `__m128` from four floating point values lowest to highest.

This matches the memory order of `__m128`, i.e., `a` will be the lowest 32 bits of the result, and `d` the highest.

    assert_eq!(__m128::new(a, b, c, d), _mm_setr_ps(a, b, c, d));

Intel’s documentation