# Function _mm256_mask_i64scatter_ps

1.89.0 · Source

    pub unsafe fn _mm256_mask_i64scatter_ps(
        base_addr: *mut f32,
        k: __mmask8,
        vindex: __m256i,
        a: __m128,
        const SCALE: i32,
    )

Available on (x86 or x86-64) and target feature `avx512f` and target feature `avx512vl` and x86-64 only.
Expand description

Stores 4 single-precision (32-bit) floating-point elements from a to memory starting at location base_addr at packed 64-bit integer indices stored in vindex scaled by scale using writemask k (elements whose corresponding mask bit is not set are not written to memory).

Intel’s documentation