# Function _mm512_mask_i32scatter_ps

1.89.0 · Source

    pub unsafe fn _mm512_mask_i32scatter_ps(
        slice: *mut f32,
        mask: __mmask16,
        offsets: __m512i,
        src: __m512,
        const SCALE: i32,
    )

Available on (x86 or x86-64) and target feature `avx512f` and x86 only.
Expand description

Scatter single-precision (32-bit) floating-point elements from a into memory using 32-bit indices. 32-bit elements are stored at addresses starting at base_addr and offset by each 32-bit element in vindex (each index is scaled by the factor in scale) subject to mask k (elements are not stored when the corresponding mask bit is not set). scale should be 1, 2, 4 or 8.

Intel’s documentation