# Function _mm256_maskz_broadcastss_ps

1.89.0 · Source

    pub fn _mm256_maskz_broadcastss_ps(k: __mmask8, a: __m128) -> __m256

Available on (x86 or x86-64) and target feature `avx512f` and target feature `avx512vl` and x86 only.
Expand description

Broadcast the low single-precision (32-bit) floating-point element from a to all elements of dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation